0.1.0 - ci-build

AnamnesiinRemoto - Local Development build (v0.1.0) built by the FHIR (HL7® FHIR® Standard) Build Tools. See the Directory of published versions

## Data Type Profile: TimingPianoCura

Official URL: http://anamnesi.na.icar.cnr/StructureDefinition/TimingPianoCura | Version: 0.1.0
Active as of 2025-06-26 | Computable Name: TimingPianoCura

Descrizione dei campi da valorizzare in Timing

Usage:

- This DataType Constraint is not used by any profiles in this Implementation Guide

### Formal Views of Profile Content

Description of Profiles, Differentials, Snapshots and how the different presentations work.

- Key Elements Table
- Differential Table
- Snapshot Table
- Statistics/References
- All

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Timing |  | 0..* | Timing | A timing schedule that specifies an event that may occur multiple times ele-1: All FHIR elements must have a @value or children
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
Documentation for this format

#### Constraints

Id | Grade | Path(s) | Details | Requirements
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both : extension.exists() != value.exists() |

This structure is derived from Timing

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Timing |  | 0..* | Timing | A timing schedule that specifies an event that may occur multiple times
repeat |  |  |  |
count |  | 0..1 | positiveInt | Numero di cicli
duration |  | 0..1 | decimal | Durata del ciclo
frequency |  | 0..1 | positiveInt | Frequenza
timeOfDay |  | 0..* | time | Orario
Documentation for this format

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Timing |  | 0..* | Timing | A timing schedule that specifies an event that may occur multiple times
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
event | Σ | 0..* | dateTime | When the event occurs
repeat | Σ C | 0..1 | Element | When the event is to occur tim-1: if there's a duration, there needs to be duration units tim-2: if there's a period, there needs to be period units tim-4: duration SHALL be a non-negative value tim-5: period SHALL be a non-negative value tim-6: If there's a periodMax, there must be a period tim-7: If there's a durationMax, there must be a duration tim-8: If there's a countMax, there must be a count tim-9: If there's an offset, there must be a when (and not C, CM, CD, CV) tim-10: If there's a timeOfDay, there cannot be a when, or vice versa
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
bounds[x] | Σ | 0..1 |  | Length/Range of lengths, or (Start and/or end) limits
boundsDuration |  |  | Duration |
boundsRange |  |  | Range |
boundsPeriod |  |  | Period |
count | Σ | 0..1 | positiveInt | Numero di cicli
countMax | Σ | 0..1 | positiveInt | Maximum number of times to repeat
duration | Σ | 0..1 | decimal | Durata del ciclo
durationMax | Σ | 0..1 | decimal | How long when it happens (Max)
durationUnit | Σ | 0..1 | code | s | min | h | d | wk | mo | a - unit of time (UCUM) Binding: UnitsOfTime (required): A unit of time (units from UCUM).
frequency | Σ | 0..1 | positiveInt | Frequenza
frequencyMax | Σ | 0..1 | positiveInt | Event occurs up to frequencyMax times per period
period | Σ | 0..1 | decimal | Event occurs frequency times per period
periodMax | Σ | 0..1 | decimal | Upper limit of period (3-4 hours)
periodUnit | Σ | 0..1 | code | s | min | h | d | wk | mo | a - unit of time (UCUM) Binding: UnitsOfTime (required): A unit of time (units from UCUM).
dayOfWeek | Σ | 0..* | code | mon | tue | wed | thu | fri | sat | sun Binding: DaysOfWeek (required)
timeOfDay | Σ | 0..* | time | Orario
when | Σ | 0..* | code | Code for time period of occurrence Binding: EventTiming (required): Real world event relating to the schedule.
offset | Σ | 0..1 | unsignedInt | Minutes from event (before or after)
code | Σ | 0..1 | CodeableConcept | BID | TID | QID | AM | PM | QD | QOD | + Binding: TimingAbbreviation (preferred): Code for a known / defined timing pattern.
Documentation for this format

#### Terminology Bindings

Path | Conformance | ValueSet | URI
Timing.repeat.durationUnit | required | UnitsOfTime `http://hl7.org/fhir/ValueSet/units-of-time|4.0.1` from the FHIR Standard
Timing.repeat.periodUnit | required | UnitsOfTime `http://hl7.org/fhir/ValueSet/units-of-time|4.0.1` from the FHIR Standard
Timing.repeat.dayOfWeek | required | DaysOfWeek `http://hl7.org/fhir/ValueSet/days-of-week|4.0.1` from the FHIR Standard
Timing.repeat.when | required | EventTiming `http://hl7.org/fhir/ValueSet/event-timing|4.0.1` from the FHIR Standard
Timing.code | preferred | TimingAbbreviation `http://hl7.org/fhir/ValueSet/timing-abbreviation` from the FHIR Standard

#### Constraints

Id | Grade | Path(s) | Details | Requirements
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
tim-1 | error | Timing.repeat | if there's a duration, there needs to be duration units : duration.empty() or durationUnit.exists() |
tim-2 | error | Timing.repeat | if there's a period, there needs to be period units : period.empty() or periodUnit.exists() |
tim-4 | error | Timing.repeat | duration SHALL be a non-negative value : duration.exists() implies duration >= 0 |
tim-5 | error | Timing.repeat | period SHALL be a non-negative value : period.exists() implies period >= 0 |
tim-6 | error | Timing.repeat | If there's a periodMax, there must be a period : periodMax.empty() or period.exists() |
tim-7 | error | Timing.repeat | If there's a durationMax, there must be a duration : durationMax.empty() or duration.exists() |
tim-8 | error | Timing.repeat | If there's a countMax, there must be a count : countMax.empty() or count.exists() |
tim-9 | error | Timing.repeat | If there's an offset, there must be a when (and not C, CM, CD, CV) : offset.empty() or (when.exists() and ((when in ('C' | 'CM' | 'CD' | 'CV')).not())) |
tim-10 | error | Timing.repeat | If there's a timeOfDay, there cannot be a when, or vice versa : timeOfDay.empty() or when.empty() |

This structure is derived from Timing

Summary

Key Elements View

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Timing |  | 0..* | Timing | A timing schedule that specifies an event that may occur multiple times ele-1: All FHIR elements must have a @value or children
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
Documentation for this format

#### Constraints

Id | Grade | Path(s) | Details | Requirements
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both : extension.exists() != value.exists() |

Differential View

This structure is derived from Timing

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Timing |  | 0..* | Timing | A timing schedule that specifies an event that may occur multiple times
repeat |  |  |  |
count |  | 0..1 | positiveInt | Numero di cicli
duration |  | 0..1 | decimal | Durata del ciclo
frequency |  | 0..1 | positiveInt | Frequenza
timeOfDay |  | 0..* | time | Orario
Documentation for this format

Snapshot View

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Timing |  | 0..* | Timing | A timing schedule that specifies an event that may occur multiple times
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
event | Σ | 0..* | dateTime | When the event occurs
repeat | Σ C | 0..1 | Element | When the event is to occur tim-1: if there's a duration, there needs to be duration units tim-2: if there's a period, there needs to be period units tim-4: duration SHALL be a non-negative value tim-5: period SHALL be a non-negative value tim-6: If there's a periodMax, there must be a period tim-7: If there's a durationMax, there must be a duration tim-8: If there's a countMax, there must be a count tim-9: If there's an offset, there must be a when (and not C, CM, CD, CV) tim-10: If there's a timeOfDay, there cannot be a when, or vice versa
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
bounds[x] | Σ | 0..1 |  | Length/Range of lengths, or (Start and/or end) limits
boundsDuration |  |  | Duration |
boundsRange |  |  | Range |
boundsPeriod |  |  | Period |
count | Σ | 0..1 | positiveInt | Numero di cicli
countMax | Σ | 0..1 | positiveInt | Maximum number of times to repeat
duration | Σ | 0..1 | decimal | Durata del ciclo
durationMax | Σ | 0..1 | decimal | How long when it happens (Max)
durationUnit | Σ | 0..1 | code | s | min | h | d | wk | mo | a - unit of time (UCUM) Binding: UnitsOfTime (required): A unit of time (units from UCUM).
frequency | Σ | 0..1 | positiveInt | Frequenza
frequencyMax | Σ | 0..1 | positiveInt | Event occurs up to frequencyMax times per period
period | Σ | 0..1 | decimal | Event occurs frequency times per period
periodMax | Σ | 0..1 | decimal | Upper limit of period (3-4 hours)
periodUnit | Σ | 0..1 | code | s | min | h | d | wk | mo | a - unit of time (UCUM) Binding: UnitsOfTime (required): A unit of time (units from UCUM).
dayOfWeek | Σ | 0..* | code | mon | tue | wed | thu | fri | sat | sun Binding: DaysOfWeek (required)
timeOfDay | Σ | 0..* | time | Orario
when | Σ | 0..* | code | Code for time period of occurrence Binding: EventTiming (required): Real world event relating to the schedule.
offset | Σ | 0..1 | unsignedInt | Minutes from event (before or after)
code | Σ | 0..1 | CodeableConcept | BID | TID | QID | AM | PM | QD | QOD | + Binding: TimingAbbreviation (preferred): Code for a known / defined timing pattern.
Documentation for this format

#### Terminology Bindings

Path | Conformance | ValueSet | URI
Timing.repeat.durationUnit | required | UnitsOfTime `http://hl7.org/fhir/ValueSet/units-of-time|4.0.1` from the FHIR Standard
Timing.repeat.periodUnit | required | UnitsOfTime `http://hl7.org/fhir/ValueSet/units-of-time|4.0.1` from the FHIR Standard
Timing.repeat.dayOfWeek | required | DaysOfWeek `http://hl7.org/fhir/ValueSet/days-of-week|4.0.1` from the FHIR Standard
Timing.repeat.when | required | EventTiming `http://hl7.org/fhir/ValueSet/event-timing|4.0.1` from the FHIR Standard
Timing.code | preferred | TimingAbbreviation `http://hl7.org/fhir/ValueSet/timing-abbreviation` from the FHIR Standard

#### Constraints

Id | Grade | Path(s) | Details | Requirements
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
tim-1 | error | Timing.repeat | if there's a duration, there needs to be duration units : duration.empty() or durationUnit.exists() |
tim-2 | error | Timing.repeat | if there's a period, there needs to be period units : period.empty() or periodUnit.exists() |
tim-4 | error | Timing.repeat | duration SHALL be a non-negative value : duration.exists() implies duration >= 0 |
tim-5 | error | Timing.repeat | period SHALL be a non-negative value : period.exists() implies period >= 0 |
tim-6 | error | Timing.repeat | If there's a periodMax, there must be a period : periodMax.empty() or period.exists() |
tim-7 | error | Timing.repeat | If there's a durationMax, there must be a duration : durationMax.empty() or duration.exists() |
tim-8 | error | Timing.repeat | If there's a countMax, there must be a count : countMax.empty() or count.exists() |
tim-9 | error | Timing.repeat | If there's an offset, there must be a when (and not C, CM, CD, CV) : offset.empty() or (when.exists() and ((when in ('C' | 'CM' | 'CD' | 'CV')).not())) |
tim-10 | error | Timing.repeat | If there's a timeOfDay, there cannot be a when, or vice versa : timeOfDay.empty() or when.empty() |

This structure is derived from Timing

Summary

Other representations of profile: CSV, Excel, Schematron